Protel Design System Design Rule Check
PCB File : D:\FER\Diplomski\4 Semestar\Diplomski\Altium\mali_u_veliki\SSOP2PDIP.PcbDoc
Date     : 1.6.2015.
Time     : 22:18:10

Processing Rule : Net Antennae (Tolerance=0mil) (All)
Rule Violations :0

Processing Rule : Silk to Silk (Clearance=10mil) (All),(All)
   Violation between Text "U4" (4344mil,3034mil)  Bottom Overlay and 
                     Track (4350mil,3010mil)(4350mil,3090mil)  Bottom Overlay
   Violation between Text "U4" (4344mil,3034mil)  Bottom Overlay and 
                     Track (4350mil,3110mil)(4350mil,3190mil)  Bottom Overlay
   Violation between Text "U4" (4344mil,3034mil)  Bottom Overlay and 
                     Track (4350mil,3090mil)(4350mil,3110mil)  Bottom Overlay
   Violation between Text "U4" (4344mil,3034mil)  Bottom Overlay and 
                     Track (4250mil,3010mil)(4250mil,3190mil)  Bottom Overlay
   Violation between Text "U2" (3744mil,3034mil)  Bottom Overlay and 
                     Track (3750mil,3010mil)(3750mil,3090mil)  Bottom Overlay
   Violation between Text "U2" (3744mil,3034mil)  Bottom Overlay and 
                     Track (3750mil,3110mil)(3750mil,3190mil)  Bottom Overlay
   Violation between Text "U2" (3744mil,3034mil)  Bottom Overlay and 
                     Track (3750mil,3090mil)(3750mil,3110mil)  Bottom Overlay
   Violation between Text "U2" (3744mil,3034mil)  Bottom Overlay and 
                     Track (3650mil,3010mil)(3650mil,3190mil)  Bottom Overlay
Rule Violations :8

Processing Rule : Silk To Solder Mask (Clearance=10mil) (IsPad),(All)
   Violation between Text "U4" (4344mil,3034mil)  Bottom Overlay and 
                     Pad U3-2(4300mil,3050mil)  Multi-Layer
   Violation between Text "U2" (3744mil,3034mil)  Bottom Overlay and 
                     Pad U1-2(3700mil,3050mil)  Multi-Layer
Rule Violations :2

Processing Rule : Minimum Solder Mask Sliver (Gap=10mil) (All),(All)
   Violation between Pad U5-7(4066.75mil,3012.795mil)  Top Layer and 
                     Pad U5-8(4066.75mil,3038.386mil)  Top Layer
   Violation between Pad U5-6(4066.75mil,2987.205mil)  Top Layer and 
                     Pad U5-7(4066.75mil,3012.795mil)  Top Layer
   Violation between Pad U5-5(4066.75mil,2961.614mil)  Top Layer and 
                     Pad U5-6(4066.75mil,2987.205mil)  Top Layer
   Violation between Pad U5-3(3933.25mil,2987.205mil)  Top Layer and 
                     Pad U5-4(3933.25mil,2961.614mil)  Top Layer
   Violation between Pad U5-2(3933.25mil,3012.795mil)  Top Layer and 
                     Pad U5-3(3933.25mil,2987.205mil)  Top Layer
   Violation between Pad U5-1(3933.25mil,3038.386mil)  Top Layer and 
                     Pad U5-2(3933.25mil,3012.795mil)  Top Layer
Rule Violations :6

Processing Rule : Hole To Hole Clearance (Gap=10mil) (All),(All)
Rule Violations :0

Processing Rule : Hole Size Constraint (Min=1mil) (Max=100mil) (All)
Rule Violations :0

Processing Rule : Height Constraint (Min=0mil) (Max=1000mil) (Prefered=500mil) (All)
Rule Violations :0

Processing Rule : Width Constraint (Min=10mil) (Max=10mil) (Preferred=10mil) (All)
Rule Violations :0

Processing Rule : Power Plane Connect Rule(Relief Connect )(Expansion=20mil) (Conductor Width=10mil) (Air Gap=10mil) (Entries=4) (All)
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=10mil) (All),(All)
Rule Violations :0

Processing Rule : Un-Routed Net Constraint ( (All) )
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
Rule Violations :0


Violations Detected : 16
Time Elapsed        : 00:00:00