Added Component: Designator=C1(CAP_2)
Added Component: Designator=C2(CAP_2)
Added Component: Designator=U1(Arduino Micro)
Added Component: Designator=U2(HDR1X5)
Added Component: Designator=U3(DCT_8)
Added Component: Designator=U4(TO220ABN)
Added Pin To Net: NetName=GND Pin=C1-0
Added Pin To Net: NetName=+12V Pin=C1-1
Added Pin To Net: NetName=GND Pin=C2-0
Added Pin To Net: NetName=+5V Pin=C2-1
Added Pin To Net: NetName=AX12_DATA Pin=U1-2
Added Pin To Net: NetName=AX12_DATA Pin=U1-3
Added Pin To Net: NetName=SDA1 Pin=U1-6
Added Pin To Net: NetName=SCL1 Pin=U1-7
Added Pin To Net: NetName=SOWTFARE_RX Pin=U1-14
Added Pin To Net: NetName=SOFTWARE_TX Pin=U1-15
Added Pin To Net: NetName=+3.3V Pin=U1-18
Added Pin To Net: NetName=GND Pin=U1-30
Added Pin To Net: NetName=+5V Pin=U1-31
Added Pin To Net: NetName=¸EOC Pin=U2-1
Added Pin To Net: NetName=SDA2 Pin=U2-2
Added Pin To Net: NetName=+3.3V Pin=U2-3
Added Pin To Net: NetName=SCL2 Pin=U2-4
Added Pin To Net: NetName=GND Pin=U2-5
Added Pin To Net: NetName=GND Pin=U3-1
Added Pin To Net: NetName=+5V Pin=U3-2
Added Pin To Net: NetName=SCL1 Pin=U3-3
Added Pin To Net: NetName=SDA1 Pin=U3-4
Added Pin To Net: NetName=SDA2 Pin=U3-5
Added Pin To Net: NetName=SCL2 Pin=U3-6
Added Pin To Net: NetName=+3.3V Pin=U3-7
Added Pin To Net: NetName=+12V Pin=U4-1
Added Pin To Net: NetName=+5V Pin=U4-2
Added Pin To Net: NetName=GND Pin=U4-3
Added Member To Class: ClassName=Sonda Member=Component C1 Cap
Added Member To Class: ClassName=Sonda Member=Component C2 Cap
Added Member To Class: ClassName=Sonda Member=Component U1 Arduino_Micro
Added Member To Class: ClassName=Sonda Member=Component U2 Keller_7LD_pressure_transducer
Added Member To Class: ClassName=Sonda Member=Component U3 PCA9306
Added Member To Class: ClassName=Sonda Member=Component U4 L7805CV
Added Room: Name=Sonda
