;###########################################################################
;# 
;# Copyright 2004-2005, Copyright (c) ATMEL Germany GmbH.  All rights reserved.
;# 
;# Installation inf for the ATMEL GPS chipset with USB interface.
;# 
;# Filename:	atmelUSB.inf
;# Abstract:	Windows 9x/ME/2000/XP installation file for ATMEL
;# 		GPS devices, based on ANTARIS MK II technology,
;# 		providing a USB interface.
;# Last Update:	August 23, 2004 (Version 0.0.1.0)
;# Change Log:	00/00/00 - fill
;# 
;##########################################################################
;
[Version]
Signature = "$CHICAGO$"
Class = Ports
ClassGUID = {4D36E978-E325-11CE-BFC1-08002BE10318}
Provider = %atmel%
LayoutFile = Layout.inf,Layout1.inf,Layout2.inf
DriverVer=10/05/2005,0.0.5.0


[DestinationDirs]
DefaultDestDir = 10,system32\drivers; Good for all OSs: "%windir%\system32\drivers"


[ControlFlags]
ExcludeFromSelect = *


[Manufacturer]
%atmel% = atmel.Models


[atmel.Models]
;%ANTARIS4.Descr% = ANTARIS4,USB\VID_0E8D&PID_3329
;%ANTARIS4.Descr% = ANTARIS4,USB\VID_1546&PID_01A4&MI_01
%ANTARIS4.Descr% = ANTARIS4,USB\VID_1546&PID_01A4
%ANTARIS4_03.Descr% = ANTARIS4,USB\VID_0E8D&PID_3329
%ANTARIS4_05.Descr% = ANTARIS4,USB\VID_1546&PID_05A4
%ANTARIS4_07.Descr% = ANTARIS4,USB\VID_1546&PID_07A4
%ANTARIS4_09.Descr% = ANTARIS4,USB\VID_1546&PID_09A4
%ANTARIS4_0B.Descr% = ANTARIS4,USB\VID_1546&PID_0BA4
%ANTARIS4_0D.Descr% = ANTARIS4,USB\VID_1546&PID_0DA4
%ANTARIS4_0F.Descr% = ANTARIS4,USB\VID_1546&PID_0FA4


[ANTARIS4]
AddReg = ANTARIS4.AddReg
CopyFiles = ANTARIS4.Copy


[ANTARIS4.NT]
AddReg = ANTARIS4.AddReg.NT
CopyFiles = ANTARIS4.Copy.NT


[ANTARIS4.Services]
;AddService = usbser, 0x00000002, ANTARIS4.Services.Install


[ANTARIS4.NT.Services]
AddService = usbser, 0x00000002, ANTARIS4.Services.Install


[ANTARIS4.Services.Install]
DisplayName = %ANTARIS4.Descr%
ServiceType = 1		; SERVICE_KERNEL_DRIVER
StartType = 3		; SERVICE_DEMAND_START
ErrorControl = 1	; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\usbser.sys
LoadOrderGroup = Base 


[ANTARIS4.AddReg]
HKR,,DevLoader,0,*ntkern
HKR,,NTMPDriver,,"usbser.sys,ccport.sys"
HKR,,AttachedTo,,COM5
HKR,,EnumPropPages,,"serialui.dll,EnumPropPages"


[ANTARIS4.AddReg.NT]
HKR,,AttachedTo,,COM5
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
;HKR,,ConfigDialog,,serialui.dll


[ANTARIS4.Copy]
usbser.sys,,,
ntkern.vxd,,,
ccport.sys,,,



[ANTARIS4.Copy.NT]
usbser.sys


[Strings]
atmel   = "ATMEL Germany GmbH"
ANTARIS4.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfg1)"
ANTARIS4_03.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfg3)"
ANTARIS4_05.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfg5)"
ANTARIS4_07.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfg7)"
ANTARIS4_09.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfg9)"
ANTARIS4_0B.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfgB)"
ANTARIS4_0D.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfgD)"
ANTARIS4_0F.Descr = "Atmel ANTARIS(r) 4  -  GPS Receiver (cfgF)"

