HI-TECH Software C Compiler 

Linker command line:

--edf=C:\Program Files (x86)\HI-TECH Software\PICC\9.83\dat\en_msgs.txt -cs \
  -h+Zadatak 2.sym -z -Q16F690 -ol.obj -MZadatak 2.map -E1 \
  -ACONST=00h-0FFhx16 -ACODE=00h-07FFhx2 -ASTRCODE=00h-0FFFh \
  -AENTRY=00h-0FFhx16 -ASTRING=00h-0FFhx16 -ABANK0=020h-06Fh \
  -ABANK1=0A0h-0EFh -ABANK2=0120h-016Fh \
  -ARAM=020h-06Fh,0A0h-0EFh,0120h-016Fh \
  -AABS1=020h-07Fh,0A0h-0EFh,0120h-016Fh -ACOMMON=070h-07Fh -ASFR0=00h-01Fh \
  -ASFR1=080h-09Fh -ASFR2=0100h-011Fh -ASFR3=0180h-01EFh \
  -preset_vec=00h,intentry,init,end_init -ppowerup=CODE -pfunctab=CODE \
  -ACONFIG=02007h-02007h -pconfig=CONFIG -DCONFIG=2 -AIDLOC=02000h-02003h \
  -pidloc=IDLOC -DIDLOC=2 -AEEDATA=00h-0FFh/02100h -peeprom_data=EEDATA \
  -DEEDATA=2 -DCODE=2 -DSTRCODE=2 -DSTRING=2 -DCONST=2 -DENTRY=2 -k \
  startup.obj Zadatak 2.obj 

Object code version is 3.10

Machine type is 16F690



                Name                               Link     Load   Length Selector   Space Scale
startup.obj     end_init                              0        0        2        0       0
Zadatak 2.obj   config                             2007     2007        1     400E       0
                text123                             70E      70E       12      E1C       0
                text122                             700      700        E      E00       0
                text121                             720      720       1A      E40       0
                text120                             73A      73A       25      E74       0
                text119                             75F      75F       33      EBE       0
                maintext                            792      792       6E      F24       0
                cstackCOMMON                         70       70        A       70       1
                cinit                               6FD      6FD        3      DFA       0
                strings                               2        2       61        4       0

TOTAL           Name                               Link     Load   Length     Space
        CLASS   CONST          

        CLASS   CODE           
                end_init                              0        0        2         0
                text123                             70E      70E       12         0
                text122                             700      700        E         0
                text121                             720      720       1A         0
                text120                             73A      73A       25         0
                text119                             75F      75F       33         0
                maintext                            792      792       6E         0
                cinit                               6FD      6FD        3         0

        CLASS   STRCODE        

        CLASS   ENTRY          

        CLASS   STRING         
                strings                               2        2       61         0

        CLASS   BANK0          

        CLASS   BANK1          

        CLASS   BANK2          

        CLASS   RAM            

        CLASS   ABS1           
                abs_s1                               7E       7E        2         1

        CLASS   COMMON         
                cstackCOMMON                         70       70        A         1

        CLASS   SFR0           

        CLASS   SFR1           

        CLASS   SFR2           

        CLASS   SFR3           

        CLASS   CONFIG         
                config                             2007     2007        1         0

        CLASS   IDLOC          

        CLASS   EEDATA         

        CLASS   BANK3          



SEGMENTS        Name                           Load    Length   Top    Selector   Space  Class     Delta

                reset_vec                      000000  000002  000002         0       0  CODE        2
                strings                        000002  000061  000063         4       0  STRING      2
                cstackCOMMON                   000070  00000A  00007A        70       1  COMMON      1
                cinit                          0006FD  000003  000700       DFA       0  CODE        2
                text122                        000700  00000E  00070E       E00       0  CODE        2
                text123                        00070E  000012  000720       E1C       0  CODE        2
                text121                        000720  00001A  00073A       E40       0  CODE        2
                text120                        00073A  000025  00075F       E74       0  CODE        2
                text119                        00075F  000033  000792       EBE       0  CODE        2
                maintext                       000792  00006E  000800       F24       0  CODE        2
                config                         002007  000001  002008      400E       0  CONFIG      2


UNUSED ADDRESS RANGES

        Name                Unused          Largest block    Delta
        BANK0            0020-006F             50           1
        BANK1            00A0-00EF             50           1
        BANK2            0120-016F             50           1
        CODE             0063-06FC            69A           2
                         0800-0FFF            800
        COMMON           007A-007D              4           1
        CONST            0063-06FC            100           2
                         0800-0FFF            100
        EEDATA           2100-21FF            100           2
        ENTRY            0063-06FC            100           2
                         0800-0FFF            100
        IDLOC            2000-2003              4           2
        RAM              0020-006F             50           1
                         00A0-00EF             50
                         0120-016F             50
        SFR0             0000-001F             20           1
        SFR1             0080-009F             20           1
        SFR2             0100-011F             20           1
        SFR3             0180-01EF             70           1
        STRCODE          0063-06FC            69A           2
                         0800-0FFF            800
        STRING           0063-06FC            100           2
                         0800-0FFF            100

                                  Symbol Table

??_main                   cstackCOMMON 0076
??_rs232_init             cstackCOMMON 0070
??_rs232_read_byte        cstackCOMMON 0070
??_rs232_send_byte        cstackCOMMON 0070
??_rs232_send_text        cstackCOMMON 0071
??_start                  cstackCOMMON 0072
?_main                    cstackCOMMON 0070
?_rs232_init              cstackCOMMON 0070
?_rs232_read_byte         cstackCOMMON 0070
?_rs232_send_byte         cstackCOMMON 0070
?_rs232_send_text         cstackCOMMON 0070
?_start                   cstackCOMMON 0070
_ANSEL                    (abs)        011E
_ANSELH                   (abs)        011F
_CARRY                    (abs)        0018
_CREN                     (abs)        00C4
_EEADR                    (abs)        010D
_EECON1                   (abs)        018C
_EECON2                   (abs)        018D
_EEDATA                   (abs)        010C
_FERR                     (abs)        00C2
_GIE                      (abs)        005F
_OERR                     (abs)        00C1
_PORTB                    (abs)        0006
_PORTC                    (abs)        0007
_RA3                      (abs)        002B
_RCIF                     (abs)        0065
_RCREG                    (abs)        001A
_RCSTA                    (abs)        0018
_RD                       (abs)        0C60
_SPBRG                    (abs)        0099
_TRISA                    (abs)        0085
_TRISB                    (abs)        0086
_TRISC                    (abs)        0087
_TRMT                     (abs)        04C1
_TXREG                    (abs)        0019
_TXSTA                    (abs)        0098
_WR                       (abs)        0C61
_WREN                     (abs)        0C62
__Habs1                   abs1         0000
__Hbank0                  bank0        0000
__Hbank1                  bank1        0000
__Hbank2                  bank2        0000
__Hbank3                  bank3        0000
__Hcinit                  cinit        0000
__Hclrtext                clrtext      0000
__Hcode                   code         0000
__Hcommon                 common       0000
__Hconfig                 config       2008
__HcstackCOMMON           cstackCOMMON 0000
__Heeprom_data            eeprom_data  0000
__Hend_init               end_init     0002
__Hfunctab                functab      0000
__Hidloc                  idloc        0000
__Hinit                   init         0000
__Hintentry               intentry     0000
__Hmaintext               maintext     0000
__Hpowerup                powerup      0000
__Hram                    ram          0000
__Hreset_vec              reset_vec    0000
__Hsfr0                   sfr0         0000
__Hsfr1                   sfr1         0000
__Hsfr2                   sfr2         0000
__Hsfr3                   sfr3         0000
__Hstrings                strings      0000
__Htext                   text         0000
__Labs1                   abs1         0000
__Lbank0                  bank0        0000
__Lbank1                  bank1        0000
__Lbank2                  bank2        0000
__Lbank3                  bank3        0000
__Lcinit                  cinit        0000
__Lclrtext                clrtext      0000
__Lcode                   code         0000
__Lcommon                 common       0000
__Lconfig                 config       2007
__LcstackCOMMON           cstackCOMMON 0000
__Leeprom_data            eeprom_data  0000
__Lend_init               end_init     0000
__Lfunctab                functab      0000
__Lidloc                  idloc        0000
__Linit                   init         0000
__Lintentry               intentry     0000
__Lmaintext               maintext     0000
__Lpowerup                powerup      0000
__Lram                    ram          0000
__Lreset_vec              reset_vec    0000
__Lsfr0                   sfr0         0000
__Lsfr1                   sfr1         0000
__Lsfr2                   sfr2         0000
__Lsfr3                   sfr3         0000
__Lstrings                strings      0000
__Ltext                   text         0000
__S0                      (abs)        2008
__S1                      (abs)        007A
__S2                      (abs)        0000
__end_of_main             maintext     0800
__end_of_rs232_init       text123      0720
__end_of_rs232_read_byte  text121      073A
__end_of_rs232_send_byte  text122      070E
__end_of_rs232_send_text  text120      075F
__end_of_start            text119      0792
__pcstackCOMMON           cstackCOMMON 0070
__pmaintext               maintext     0792
__pstrings                strings      0002
__ptext118                text118      0000
__ptext119                text119      075F
__ptext120                text120      073A
__ptext121                text121      0720
__ptext122                text122      0700
__ptext123                text123      070E
__ptext124                text124      0000
__size_of_main            (abs)        0000
__size_of_rs232_init      (abs)        0000
__size_of_rs232_read_byte (abs)        0000
__size_of_rs232_send_byte (abs)        0000
__size_of_rs232_send_text (abs)        0000
__size_of_start           (abs)        0000
_exit                     init         0000
_main                     maintext     0792
_rs232_init               text123      070E
_rs232_read_byte          text121      0720
_rs232_send_byte          text122      0700
_rs232_send_text          text120      073A
_start                    text119      075F
btemp                     (abs)        007E
end_of_initialization     cinit        06FD
intlevel0                 functab      0000
intlevel1                 functab      0000
intlevel2                 functab      0000
intlevel3                 functab      0000
intlevel4                 functab      0000
intlevel5                 functab      0000
main@temp                 cstackCOMMON 0079
reset_vec                 reset_vec    0000
rs232_send_byte@x         cstackCOMMON 0070
rs232_send_text@c         cstackCOMMON 0072
rs232_send_text@i         cstackCOMMON 0073
rs232_send_text@string    cstackCOMMON 0075
start                     init         0000
start@i                   cstackCOMMON 0074
start@x                   cstackCOMMON 0070
start_initialization      cinit        06FD
wtemp0                    (abs)        007E
